**Signal Safe FR Hydraulic 46 Fluid**

|  |
| --- |
| Product Application: |

Signal Safe FR Hydraulic 46 Fluid is a red water glycol that is used in a wide variety of industrial hydraulic systems. It is carefully formulated with anti-wear additives, corrosion inhibitors and antifreeze additives.

 Signal Safe FR Hydraulic 46 Fluid is approved by Factory Mutual Corporation Group 1-HF-1) Fluid.

Signal Safe FR Hydraulic 46 Fluid will perform in a variety of hydraulic pumps within rated conditions:

\*Vickers Vane Pumps

\*Tyrone Gear Pumps with flooded intake

\*Racine Vane Pumps with sleeve bearings

\*Denison Vane Pumps

\*Denison Piston Pumps

\*DeLaval Imo Screw Pumps

|  |
| --- |
| Package Size:  |

Drums, Pails

|  |
| --- |
| Typical Characteristics:  |

Viscosity, ASTM D 445

cSt 40°C 41.5

Viscosity Index, ASTM D 2270 175

Specific Gravity, ASTM D 1298, 15.6°C/15.6°C 1.089

Pour Point, °C, ASTM D 97 -30

Water Content, ASTM D 1744 43

PH 9.5

Color, visual Red

Visit us at – www.beaconlubricants.com