**Signal Tech H1 Chain / Guide Lubricant**

|  |
| --- |
| Product Application: |

Signal Tech H1 Chain / Guide Lubricant is specially developed, food grade chain lubricant blended from biosynthetic base oils and fortified with synthetic food grade additives. This unique formula maintains its lubricating properties to temperatures exceeding 350 ° C.

Signal Tech H1 Chain / Guide Lubricant is formulated with a natural self-cleaning property which cleans the buildup on chains attributable to the use of less adequate chain lubricants. This superior chain lubricant provides excellent protection against wear, rust, oxidation and corrosion.

Signal Tech H1 Chain / Guide Lubricant meets the requirements for a USDA H-1 quality lubricant and the requirement of the United States Code of Federal Regulations 21CFR 178.3570, 178.3620 (b), and 573.680 of the Unites States Food and Drug Administration’s Regulations.

|  |
| --- |
| Package Size: |

2.5 gallon containers, 5 gallon Pails, 55 gallon Drums

|  |
| --- |
| Features & Advantages: |

\*Excellent high temperature oxidation and thermal stability due to base stocks high degree of saturation and low acid number

\*Very low volatility. This results in less makeup due to evaporation loss

\*High viscosity index

\*Excellent lubricity

\*High degree of solvency to keep the chains free from deposits

\*High temperature initial smoke point

\*Uniform and complete cover of the chain

|  |
| --- |
| Typical Characterisitcs: |

ISO Grade

@ 40 ° C 150

@100° C 25.1

Flash Point, COC, °C 315°

Pour Point, °C -20°

Appearance Clear

Rust Prevention Pass

Four-Ball Wear 0.40