**Signal Trans ATF**

|  |
| --- |
| Product Application: |

Signal Trans ATF is a premium quality multi-functional industrial grade extended life transmission, gear, and hydraulic lubricant. It is developed for use in stationary industrial and machining equipment requiring a multi-purpose automatic transmission fluid.

Signal Trans ATF utilizes latest quality base stocks and technologically advanced additives to provide outstanding high temperature oxidation stability, extended life, excellent smooth operation, and superior friction durability. Thus allowing Signal Trans AFT to excel in heavy duty manufacturing and industrial equipment.

**\*Signal Trans ATF is not recommended automotive use\***

|  |
| --- |
| Performance Features |

\*Long oil life

\*Outstanding high temperature oxidation resistance

\*Superior friction durability

\*Smooth operation

|  |
| --- |
| Package Size: |

Bulk, Drums, Pails

|  |
| --- |
| Typical Characterisitcs: |

Color Red

Specific Gravity 31.4

Viscosity Index 174

Viscosity

cSt @ 100 ° C 6.8 – 8.5

cSt @ 40 ° C 37.1

cp @ -40 ° C 18400

cp @ -20 ° C 1310

SSU @ 100 ° F 189

Flash Point ° C 206

Pour Point ° F -40

Visit us at – www.beaconlubricants.com