**Beacon Multi-Purpose Automatic Transmission Fluid**

|  |
| --- |
| Product Application: |

Beacon Lubricants Multi-Purpose Automatic Transmission Fluid is a fully formulated multifunctional fluid for automatic transmissions. It is recommended for all Ford, GM and Chrysler cars, vans and light trucks. It is also recommended for import cars such as Audi, Honda, Mercedes-Benz, Nissan, Renault, Toyota and Volkswagen. Beacon Lubricants Multi-Purpose ATF is a Dexron IIIH, Mercon fluid and is approved against Detroit Diesel Allison C-4. It also meets the requirements of Caterpillar TO-2. Beacon Lubricants Multi-Purpose ATF provides oxidation stability, as measured in the GM oxidation test, resulting in cleaner transmissions and more reliable operation.

|  |
| --- |
| Performance Features  |

Faster circulating in cold weather

Excellent low temperature fluidity

Outstanding high temperature oxidation resistance

Superior friction durability

|  |
| --- |
| Package Size:  |

Bulk, Drums, Pails

|  |
| --- |
| Typical Characterisitcs: |

Color Red

Specific Gravity 31.4

Viscosity Index 174

Viscosity

 cSt @ 100 ° C 6.8 – 8.5

 cSt @ 40 ° C 37.1

 cp @ -40 ° C 18400

 cp @ -20 ° C 1310

 SSU @ 100 ° F 189

Flash Point ° C 206

Pour Point ° F -40

Visit us at – www.beaconlubricants.com