**Beacon Power Steering Fluid**

|  |
| --- |
| Product Application: |

Beacon Power Steering Fluid is blended with premium base oils and proven additive packages to provide excellent performance in power steering systems. It contains a unique friction modifier that has been shown to reduce power steering pump noise.

|  |
| --- |
| Meets or Exceeds the following Specifications: |

Volkswagen TL-VW-570-26,   
GM 9985010 Saginaw Power Steering Systems,   
GM 9985835 Wide Temperature Performance (Synthetic Multi-temperature),   
Chrysler MS-1872,   
Chrysler MS-5931,   
Chrysler 4883077,   
Chrysler 5166226AA,   
Ford M2C195-A,   
Honda PN 08206-9002 PE,   
Audi PN G002000,   
Mercedes Benz PN 009898803,   
Saab PN 30 09 800   
and Subaru PN K0Z0pA0080 requirements.

|  |
| --- |
| Package Size: |

Pails, Drums, Bulk

|  |
| --- |
| Performance Features: |

\*Promotes smooth efficient operation

\*Outstanding anti-wear properties

\*Tenaciously resists foaming while maintaining proper viscosity

\*Protects from rust, oxidation, and corrosity

|  |
| --- |
| Typical Characteristics: |

Viscosity, cSt @ 40 ° F 32.1

Viscosity, cSt @ 100 ° F 6.4

Viscosity Index 167

Flash Point, COC, ° F 380

Pour Point, ° F -30

Gravity, API 30.0

Color 1.5

Visit us at – www.beaconlubricants.com