**Signal Cut 310 Oil**

|  |
| --- |
| Product Application: |

Beacon Signal Cut 310 Oil is a cutting edge light viscosity low odor heavy duty cutting oil, ideally suited for gun drilling applications where fine finishes, high heat dissipation and maximum flush of fines is required.

Signal Cut 310 utilizes carefully selected stable base stocks and the latest sulfurized ester polymers additives to provide an excellent heavy duty cutting fluid, for ferrous and non-ferrous metals.

Due to the heavy duty component technology, Signal Cut 310 may discolor copper and its associated alloys, thus if staining is objectionable, it is not recommended for use in those situations.

|  |
| --- |
| Package Size: |

Bulk, Drums, Pails

|  |
| --- |
| Features and Advantages: |

\*Carbide Tooling Compatible

\*Excellent High Heat Dissipation Capabilities

\*Mist Suppressant Technology

\*Increased production resulting from longer tool life and reduced downtime

|  |
| --- |
| Typical Characteristics: |

Viscosity, ASTM D 445

cSt @ 40°C 15

cSt @ 100°C 3.5

Pour Point, °C, ASTM D 97 -15

Flash, °C, ASTM d 92 182

Specific Gravity @ 15°C kg/l, ASTM D 1298 0.859

Visit us at – www.beaconlubricants.com