**Signal GL1 Gear Oils**

|  |
| --- |
| Product Application: |

Signal GL1 Gear Oils are premium performance gear lubricants formulated for use in transmissions, axles, final drivers, and any application which requires an API GL-1 product. They are made from highly-refined paraffinic base stocks to provide for excellent shear and thermal stability.

|  |
| --- |
| Package Size: |

Bulk, Drums, Pails

|  |
| --- |
| Features and Advantages: |

\*Foam resistant

\*Excellent corrosion protection

\*Great compatibility with all types of seals and gaskets

\*Thermal and ox datively stable

\*Meet API GL1 requirements

|  |
| --- |
| Typical Characteristics: |

**ISO GRADE 90 140**

Viscosity, ASTM D 445

Viscosity Index (Min.) 95 95

Viscosity

cSt @ 100 ºC 17.5 31.6

cSt @ 40 ºC 198 490

Flash Point, °C, ASTM D 92 260 294

Pour Point, ºC, ASTM D 97 -6 0

Density @ 15° kg.l ASTM D 4052 0.89 0.90

**90 140**

API GL-1 \* \*