**Signal Hone 25**

|  |
| --- |
| Product Application:  |

Signal Hone 25 is an environmentally conscious medium viscosity industrial grade synthetic blend honing/cutting fluid formulated for use in all types of industrial honing, utilizing all types of honing stone mediums.

Signal Hone 25 is formulated utilizing the latest high quality pure base stocks and select chlorine and phosphorus free synthesized ester base additives to provide for unparalleled honing performance where fine papered finishes are required.

|  |
| --- |
| Package Size: |

Tote, Drum, Pail, 2 ½ gallon

|  |
| --- |
| Performance Features: |

\*Excellent settling & filterability characteristics

\*Outstanding oxidative and thermal stability

\*Formulated for all types of honing stone mediums

\*Excellent lubricity providing for exceptional finishes

|  |
| --- |
| Typical Characteristics |

Viscosity, ASTM D445

cSt @ 40°C 25.4

cSt @ 100°C 5.5

Pour Point, °C, ASTM D 97 -15

Flash, °C, ASTM D 92 182

Specific Gravity @ 15°C kg/l, ASTM D 1298 0.859

Visit us at – www.beaconlubricants.com