**Signal Marine XP Concentrate**

|  |
| --- |
| Product Application: |

Signal Marine XP Concentrate is a commercial grade extended life inhibited propylene glycol based coolant formulated for marine applications, such as closed loop cooling systems and essential winterization layups.

Signal Marine XP Concentrate is blended utilizing pure technical grade stable single phase propylene glycol then coupled with cutting edge corrosion inhibitors and acid neutralizing agents thus providing excellent corrosion protection and resistance to cavitative foaming.

|  |
| --- |
| Features and Advantages: |

\*Environmentally conscious, ecologically non-toxic – aquatic life.

\*Easily dilutable with water

\*Formulated to be safe for all marine cooling applications

\*Easily distinguishable pink color for visual & leak detection purposes

|  |
| --- |
| Package Size: |

Drums, Pails, 2 ½ gallon

|  |
| --- |
| Typical Characteristics: |

Specific Gravity(16/16°C) 1.10 – 1.15

Freezing Point, as is -37°C (-34°F)

Boiling Point (Range), Reflux 107°C – 197°C

PH, 50% Volume Solution 10.0 – 11.0

Reserve Alkalinity 3.0 – 3.8

Foam Test 150 ml. / 5sec., Max

Color Pink