**Beacon Signal Tech Power Steering Fluid**

|  |
| --- |
| Product Application: |

Beacon Signal Tech Power Steering Fluid is a premium quality full synthetic lubricant formulated to meet or exceed the warranty requirements of all major manufacturers of most automobiles and truck power steering systems.

|  |
| --- |
| Meets or Exceeds the following Specifications:  |

GM 9985010 Audi PN G002000

GM 9985835 Mercedes Benz PN 00 989 8803

Chrysler MS-1872 Saab PN 30 09 800

Chrysler MS-5931 Subaru PN K0Z09A0080

Ford M2C195-A Volkswagen P/N G002000

Honda PN 08206-9002PE Volkswagen TL VQ 570 26

Delphi 5099 Navistar TMS 6811

Hyundai PSF-3 AMC C4124

|  |
| --- |
| Package Size: |

Bulk, Drums, Pails

|  |
| --- |
| Performance Features:  |

\*Compatible with all power steering fluids

\*Minimizes sludge and varnish deposits

\*Eliminates power steering noises and whines

\*Promotes smoother, quieter performance

\*Resists foaming, oxidation, corrosion, and rusting

\*Excellent wear protection

\*Extended power steering system life

|  |
| --- |
| Typical Characteristics:  |

Kinematic Viscosity, cSt @ 100 °C, D-445 7.0

Kinematic Viscosity, cSt @ 40° C, D-445 29

Viscosity Index, (Min.) D-2270 220

Brookfield Viscosity, cP@ -40 C°, D-2983 8,700

Pour Point, D-97 -49°C

Flash Point, D-92 180°C