**Beacon Type F ATF**

|  |
| --- |
| Product Application: |

Beacon Type F ATF is an automatic transmission fluid which is formulated from high quality base oils with viscosity index improvers, antioxidants, anti-wear agents, defoamants and additives to equip the controlled frictional characteristics of a Type F fluid in automatic transmission applications.

Beacon Type F ATF is created for Ford specification M2C33-F and M2C3-G. It is recommend for use in all Ford passenger car automatic transmissions prior to the 1977 models as well as many 1977 through 1980 models.

|  |
| --- |
| Meet or Exceeds the following specifications: |

Ford M2C33-F

Ford M2C33-G

Sperry Vickers ASTM D 2882

|  |
| --- |
| Package Size: |

Bulk, Drums, Pails

|  |
| --- |
| Typical Characterisitcs: |

Color Red

Specific Gravity 31.4

Viscosity Index 150

Viscosity

cSt @ 100 ° C 7.2

cSt @ 40 ° C 36

cp @ -40 ° C 45,000

cp @ -18 ° C 1,600

Flash Point ° C 160

Pour Point ° F -40

Visit us at – www.beaconlubricants.com