**Signal Non-Detergent 50 Oil**

|  |
| --- |
| Product Application: |

Signal Non-Detergent 50 Oil is formulated for service typical of older gasoline engines operated under such mild conditions that only minimum protection afforded by compounding is desired. Oils designed for this service provide only anti-scuff capability and resistance to oil oxidation and bearing corrosion. They should not be used in any engine unless specifically recommended by the equipment manufacturer.

|  |
| --- |
| Features & Advantages: |

Formulated for service typical of older gasoline engines

|  |
| --- |
| Typical Characteristics: |

**SAE GRADE 10 20 30 40 50**

**Viscosity Index ASTM D 2270** 102 95 95 95 95

**Viscosity, ASTM d445**

**cSt @100°C** 3665.1 95.1 148 236

**cSt @40°C** 6.5 8.7 10.9 14.7 19.8