**Beacon Power Steering Fluid**

|  |
| --- |
| Product Application: |

Beacon Power Steering Fluid is blended with premium base oils and proven additive packages to provide excellent performance in power steering systems. It contains a unique friction modifier that has been shown to reduce power steering pump noise.

Beacon Power Steering Fluid meets Volkswagen TL-VW-570-26, GM 9985010 Saginaw Power Steering Systems, GM 9985835 Wide Temperature Performance (Synthetic Multi-temperature), Chrysler MS-1872, Chrysler MS-5931, Chrysler 4883077, Chrysler 5166226AA, Ford M2C195-A, Honda PN 08206-9002 PE, Audi PN G002000, Mercedes Benz PN 009898803, Saab PN 30 09 800 and Subaru PN K0Z0pA0080 requirements.

|  |
| --- |
| Package Size: |

Pails, Drums

|  |
| --- |
| Typical Characteristics:  |

Viscosity, cSt @ 40 ° F 37.8

Viscosity, cSt @ 100 ° F 7.2

Viscosity Index 142

Flash Point, COC, ° F 380

Pour Point, ° F -40

Gravity, API 30.0

Color 1.5

Visit us at – www.beaconlubricants.com