**Beacon Signal Kleen 603**

|  |
| --- |
| Product Application: |

Beacon Signal Kleen 603 is a heavy-duty industrial grade water based concentrated alkaline degreasing/cleaning agent developed to provide an excellent medium for degreasing and oil solubilizing in all types of industrial and commercial applications.

Signal Kleen 603 is specially formulated with enhanced degreasing technology enabling the product to mix to a complete, low foaming, pleasant odor, stable grease cutting solution in both hard and soft water. It is a versatile cleaner which easily dilutes to desired concentration.

|  |
| --- |
| Package Size: |

Drum, Pail, 2 ½ gallon

|  |
| --- |
| Performance Features: |

\*Pleasant citrus odor

\*Solubilizes oils and greases on contact

\*Versatile cleaner easily dilute to desired concentration

\*Formulated for all industrial degreasing applications  
\*Easily diluted with hard and/or soft water

|  |
| --- |
| Composition: |

**Appearance:** Orange

**Odor:** Citrus

**Odor threshold:** N/A

**PH: 12.5 – 13.8**

**Melting/Freezing pointing:** ~ -3°C (26.6°F)

**Boiling point and boiling range:** >100°C (212°F)

|  |
| --- |
| Dilution ratios with water: |

|  |  |
| --- | --- |
| **1-2%** | General purpose, spray bottle application for shop utility clean up. |
| **1-5%** | Industrial parts cleaning, removal of machine oils and coolant effluents. Can also be used in heated and automated, agitated, tumbling tanks with little to no foam. |
| **10-15 %** | Automatic floor scrubbers, general to heavy duty mopping, pressure washing, scrubbing vinyl, tile floors |
| **25-30%** | Degreasing, chrome soak tanks, removal of machining oils and coolants. Shop equipment/exhaust fans, tools, driveways, concrete floors |
| **40-50%** | Driveway stains, mowing equipment, underbodies, farm equipment. Heavy grease and oil stains, heavy duty degreasing, engine degreasing, floor wax removal. |

Visit us at – www.beaconlubricants.com