**Signal Tech H1 Chain / Industrial Gear 320**

|  |
| --- |
| Product Application: |

Signal Tech H1 Industrial Gear 320 is a specially developed food grade industrial gear lubricant blended from biosynthetic base oils and fortified with synthetic food grade additives.

Signal Tech H1 Industrial Gear 320 is a premium industrial food grade heavy duty gear lubricant designed for use in highly loaded bearing and gear sets encountered in industrial settings where a food grade industrial product is required.

|  |
| --- |
| Package Size: |

2.5 gallon containers, 5 gallon Pails, 55 gallon Drums

|  |
| --- |
| Features & Advantages: |

\*Excellent high temperature oxidation and thermal stability due to base stocks high degree of saturation and low acid number

\*Very low volatility. This results in less makeup due to evaporation loss

\*High viscosity index

\*Excellent lubricity

\*High degree of solvency to keep the chains free from deposits

\*High temperature initial smoke point

\*Uniform and complete cover of the chain

|  |
| --- |
| Typical Characterisitcs: |

ISO Grade

 @ 40 ° C 150

 @100° C 25.1

Flash Point, COC, °C 315°

Pour Point, °C -20°

Appearance Clear

Rust Prevention Pass

Four-Ball Wear 0.40

Visit us at – www.beaconlubricants.com