**Blue Lightning 10W-40**

|  |
| --- |
| Product Application:  |

Blue Lightning 10W-40 is a premium synthetic blend, formulated with severely hydro treated 3 group base stocks that provide outstanding, durable protection under severe, high stress and high torque conditions.

Blue Lightning 10W-40 has been optimized to help meet or exceed the unique performance characteristics demanded by motorcycle engines and offer excellent flow at low temperatures to help reduce engine wear at start-up and provide outstanding resistant to oxidation and/or volatilization at high temperatures.

|  |
| --- |
| Features and Advatages: |

\*Provides maximum protection against viscosity and thermal breakdown

\*Incredible protection against wear of engine and transmission components

\*Superior engine wear protection

\*High film strength for high revving motorcycle engines

\*Rust/Corrosion protection

|  |
| --- |
| Package Size: |

Bulk, Drums, Pails

|  |
| --- |
| Meets or Exceeds the following Specifications:  |

|  |
| --- |
| Typical Characteristics:  |