**Fyrquel R&O 220**

|  |
| --- |
| Product Application: |

Fyrquel® fluids are self-extinguishing, non-aqueous hydraulic fluids that do not support their own combustion. This self-extinguishing property exceeds the limits established for

“Less Hazardous Hydraulic Fluids” and incorporates phosphate esters’ unique true self- extinguishing property easily proven by simple flame and wick tests. Fyrquel® fireresistant

fluids reduce the risk of catastrophic fires.

|  |
| --- |
| Features and Advantages:  |

Fyrquel® fire-resistant hydraulic fluids are synthetic pure

phosphate ester fluids used in:

• Steel and aluminum furnace hydraulics;

• Die cast hydraulics;

• Reciprocating air compressors; and

• Hydraulics.

|  |
| --- |
| Package Size: |

Pails, Drums

|  |
| --- |
| Typical Characterisitcs: |

Specific Gravity @ 60 °F 1.150

Flash Point, COC, °F 475

Fire Point 530

Pour Point, °F 0

ISO Grade 46

Viscosity Index +25

Appearance amber liquid