**Signal Chiller Fluid**

|  |
| --- |
| Product Application: |

Signal Chiller Fluid is a premium quality, single phase, propylene glycol based product. It is fully fortified to safeguard against rust and corrosion. Signal Chiller Fluid is formulated as a complete ready to use product, thus no additional medium such as water are required.

|  |
| --- |
| Features and Advantages: |

\*Excellent Rust & Corrosion Protection

\*Low foam

\*Easy ready to use formula

|  |
| --- |
| Package Size: |

Pails, Drums

|  |
| --- |
| Typical Characterisitcs: |

Viscosity cSt @ 40°C 2.9

Flash Point N/A

Freeze Point °C -76

Specific Gravity 1.0381

pH 9.0

Appearance Colorless

Boiling Point 106°C