**Signal Cut 301 Oil**

|  |
| --- |
| Product Application: |

Signal Cut 301 is an environmentally friendly, cutting edge light viscosity cutting oil ideally suited for industrial band saw and gun drill applications where fine finishes, high heat dissipation and maximum flush of fines is required.

Signal Cut 301 utilizes cutting edge non staining sulfur additives, and esterized polymers to provide for an excellent multi-purpose cutting fluid and machine tool lubricant.

|  |
| --- |
| Package Size: |

Bulk, Drums, Pails

|  |
| --- |
| Features and Advantages: |

\*Carbide tooling compatible

\*Excellent high heat dissipation capabilities

\*Easily identifiable red coloring

\*Mist suppressant technology

\*Increased production resulting from longer tool life and reduced down time

|  |
| --- |
| Typical Characteristics: |

Viscosity, ASTM D 445

cSt @ 40°C 15

cSt @ 100°C 3.5

Pour Point, °C, ASTM D 97 -15

Flash, °C, ASTM D 92 182

Specific Gravity @ 15°C kg/l, ASTM D 1298 0.859

Visit us at – www.beaconlubricants.com